{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":14,"rows_kept":6,"merged":[[0,0,0,13],[2,13,5,13],[5,0,5,12]],"flags":["formulas_cached_only"]}
["衡水市园林管理局垃圾桶采购项目比选技术参数清单"]
["款式","市场调研价格","规格","材质","安装方式","筒身喷漆","标识","做工","内胆","图样","计划采购数量","单价","金额","备注"]
[1,"990元/只","1000*400*1000mm","上盖为不锈钢，不锈钢板厚度为1.5mm；桶身为镀锌钢板，板材厚度为1.5mm;装饰条为塑木条","由甲方完成垫层部分，供货方采用U型螺丝安装","桶身采用优质户外塑粉喷涂，保证三年不褪色","分类标识分可回收与不可回收，标识清晰，符合国标GB/T 19095-2008的垃圾分类标识","垃圾桶焊接牢固美观，打磨平滑，无毛刺","内胆为镀锌钢板，带提手，镀锌板厚度≥0.4mm",null,"60只",null,null,"1.采购量为计划数，具体用量按实际调整2.报价包含成品费、运费、安装费、税金等全部费用"]
[2,"920元/只","900*350*1000mm","桶身为镀锌钢板，板材厚度为1.5mm","由甲方完成垫层部分，供货方采用U型螺丝安装","桶身采用优质户外塑粉喷涂，保证三年不褪色","分类标识分可回收与不可回收，标识清晰，符合国标GB/T 19095-2008的垃圾分类标识","垃圾桶焊接牢固美观，打磨平滑，无毛刺","内胆为镀锌钢板，带提手，镀锌板厚度≥0.4mm",null,"65只"]
[3,"1100元/只","1000*400*1000mm","不锈钢，不锈钢板厚度为1.5mm","由甲方完成垫层部分，供货方采用U型螺丝安装","无","分类标识分可回收与不可回收，标识清晰","垃圾桶焊接牢固美观，打磨平滑，无毛刺","内胆为镀锌钢板，带提手，镀锌板厚度≥0.4mm",null,"75只"]
["总计（大写）："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}